<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="0.88" y1="52.64" x2="3.6" y2="63.36" width="0.1524" layer="20" curve="-30.965291"/>
<wire x1="3.6" y1="63.36" x2="6.64" y2="66.08" width="0.1524" layer="20" curve="-36.919811"/>
<wire x1="6.64" y1="66.08" x2="37.84" y2="70" width="0.1524" layer="20" curve="-32.398136"/>
<wire x1="37.84" y1="70" x2="40" y2="69.36" width="0.1524" layer="20"/>
<wire x1="40" y1="69.36" x2="47.2" y2="69.28" width="0.1524" layer="20"/>
<wire x1="47.2" y1="69.28" x2="58.8" y2="60" width="0.1524" layer="20" curve="-76.046425"/>
<wire x1="58.8" y1="60" x2="62.24" y2="50.56" width="0.1524" layer="20" curve="13.410233"/>
<wire x1="62.24" y1="50.56" x2="65.6" y2="28.64" width="0.1524" layer="20" curve="-36.024929"/>
<wire x1="65.6" y1="28.64" x2="69.2" y2="25.12" width="0.1524" layer="20" curve="109.882939"/>
<wire x1="69.2" y1="25.12" x2="74.64" y2="25.36" width="0.1524" layer="20" curve="-16.11819"/>
<wire x1="70.48" y1="20.08" x2="62.96" y2="19.12" width="0.1524" layer="20" curve="16.753422"/>
<wire x1="62.96" y1="19.12" x2="62.24" y2="17.6" width="0.1524" layer="20" curve="98.004218"/>
<wire x1="62.24" y1="17.6" x2="64" y2="11.28" width="0.1524" layer="20" curve="-16.188771"/>
<wire x1="64" y1="11.28" x2="68.64" y2="4.16" width="0.1524" layer="20" curve="51.249166"/>
<wire x1="68.64" y1="4.16" x2="68.48" y2="2.88" width="0.1524" layer="20" curve="-131.682773"/>
<wire x1="68.48" y1="2.88" x2="50.24" y2="2.88" width="0.1524" layer="20" curve="-34.067316"/>
<wire x1="50.24" y1="2.88" x2="46.8" y2="5.84" width="0.1524" layer="20" curve="-47.354374"/>
<wire x1="46.8" y1="5.84" x2="46.96" y2="6.88" width="0.1524" layer="20" curve="-68.716126"/>
<wire x1="46.96" y1="6.88" x2="51.36" y2="16.16" width="0.1524" layer="20" curve="35.473478"/>
<wire x1="51.36" y1="16.16" x2="50.24" y2="16.96" width="0.1524" layer="20" curve="124.185741"/>
<wire x1="50.24" y1="16.96" x2="48.56" y2="16.56" width="0.1524" layer="20" curve="-26.325375"/>
<wire x1="48.56" y1="16.56" x2="30" y2="18.4" width="0.1524" layer="20" curve="-11.782905"/>
<wire x1="30" y1="18.4" x2="20.64" y2="18.4" width="0.1524" layer="20" curve="23.106273"/>
<wire x1="20.64" y1="18.4" x2="16.96" y2="17.92" width="0.1524" layer="20" curve="-8.243457"/>
<wire x1="16.96" y1="17.92" x2="15.6" y2="21.76" width="0.1524" layer="20" curve="-147.614396"/>
<wire x1="15.6" y1="21.76" x2="23.28" y2="27.68" width="0.1524" layer="20" curve="3.861868"/>
<wire x1="23.28" y1="27.68" x2="25.84" y2="27.44" width="0.1524" layer="20" curve="-89.825969"/>
<wire x1="25.84" y1="27.44" x2="33.44" y2="22.24" width="0.1524" layer="20" curve="31.776831"/>
<wire x1="33.44" y1="22.24" x2="35.04" y2="24.56" width="0.1524" layer="20" curve="147.799307"/>
<wire x1="35.04" y1="24.56" x2="34.08" y2="27.6" width="0.1524" layer="20" curve="-43.563564"/>
<wire x1="34.08" y1="27.6" x2="34.48" y2="36.24" width="0.1524" layer="20" curve="3.211032"/>
<wire x1="34.48" y1="36.24" x2="35.84" y2="39.28" width="0.1524" layer="20" curve="-46.114131"/>
<wire x1="35.84" y1="39.28" x2="36" y2="42.4" width="0.1524" layer="20" curve="88.447286"/>
<wire x1="36" y1="42.4" x2="31.68" y2="44.88" width="0.1524" layer="20" curve="37.705996"/>
<wire x1="31.68" y1="44.88" x2="14.32" y2="50.64" width="0.1524" layer="20" curve="-14.699402"/>
<wire x1="14.32" y1="50.64" x2="6.24" y2="51.36" width="0.1524" layer="20" curve="41.226578"/>
<wire x1="26.543" y1="65.532" x2="20.447" y2="65.532" width="0.1524" layer="20"/>
<wire x1="20.447" y1="65.532" x2="15.367" y2="60.452" width="0.1524" layer="20" curve="90"/>
<wire x1="15.367" y1="60.452" x2="15.367" y2="59.944" width="0.1524" layer="20"/>
<wire x1="15.367" y1="59.944" x2="20.447" y2="54.864" width="0.1524" layer="20" curve="90"/>
<wire x1="20.447" y1="54.864" x2="26.543" y2="54.864" width="0.1524" layer="20"/>
<wire x1="0.88" y1="52.64" x2="1.04" y2="49.36" width="0.1524" layer="20" curve="3.094686"/>
<wire x1="1.04" y1="49.36" x2="2.56" y2="48.96" width="0.1524" layer="20" curve="141.832691"/>
<wire x1="2.56" y1="48.96" x2="6.24" y2="51.36" width="0.1524" layer="20" curve="-46.123074"/>
<wire x1="70.48" y1="20.08" x2="73.92" y2="20.08" width="0.1524" layer="20" curve="2.20341"/>
<wire x1="73.92" y1="20.08" x2="74.88" y2="20.72" width="0.1524" layer="20" curve="65.176755"/>
<wire x1="74.88" y1="20.72" x2="74.96" y2="21.04" width="0.1524" layer="20" curve="19.37045"/>
<wire x1="74.96" y1="21.04" x2="74.96" y2="24.88" width="0.1524" layer="20" curve="8.701847"/>
<wire x1="74.96" y1="24.88" x2="74.64" y2="25.36" width="0.1524" layer="20" curve="58.678406"/>
<wire x1="26.924" y1="54.356" x2="26.543" y2="54.737" width="0.1524" layer="20" curve="-90"/>
<wire x1="26.543" y1="54.737" x2="26.543" y2="54.864" width="0.1524" layer="20"/>
<wire x1="27.051" y1="66.04" x2="26.543" y2="65.532" width="0.1524" layer="20" curve="90"/>
<wire x1="26.924" y1="54.356" x2="29.21" y2="54.356" width="0.1524" layer="20"/>
<wire x1="29.21" y1="54.356" x2="29.591" y2="54.737" width="0.1524" layer="20" curve="90"/>
<wire x1="29.591" y1="54.737" x2="29.591" y2="65.659" width="0.1524" layer="20"/>
<wire x1="29.591" y1="65.659" x2="29.21" y2="66.04" width="0.1524" layer="20" curve="90"/>
<wire x1="29.21" y1="66.04" x2="27.051" y2="66.04" width="0.1524" layer="20"/>
<polygon width="0.1524" layer="46">
<vertex x="20.447" y="54.864" curve="-90"/>
<vertex x="15.367" y="59.944"/>
<vertex x="15.367" y="60.452" curve="-90"/>
<vertex x="20.447" y="65.532"/>
<vertex x="26.543" y="65.532" curve="-90"/>
<vertex x="27.051" y="66.04"/>
<vertex x="29.21" y="66.04" curve="-90"/>
<vertex x="29.591" y="65.659"/>
<vertex x="29.591" y="54.737" curve="-90"/>
<vertex x="29.21" y="54.356"/>
<vertex x="26.924" y="54.356" curve="-90"/>
<vertex x="26.543" y="54.737"/>
<vertex x="26.543" y="54.864"/>
</polygon>
<text>Long</text>
<text>Red</text>
<text>Green</text>
<text>Blue</text>
<text>Red</text>
<text>Black</text>
</plain>
<libraries>
<library name="coulston">
<packages>
<package name="0207/12">
</package>
<package name="2HEADER">
</package>
<package name="S63P">
</package>
</packages>
</library>
<library name="toucanLib">
<packages>
<package name="RGB10MM_FLAT">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="10MM" library="toucanLib" package="RGB10MM_FLAT" value="RGBLED-CARIGHT_ANGLE"/>
<element name="BLUE" library="coulston" package="0207/12" value="1kΩ"/>
<element name="GREEN" library="coulston" package="0207/12" value="1kΩ"/>
<element name="PWR" library="coulston" package="2HEADER" value="2POS_HEADERJUMPER"/>
<element name="RED" library="coulston" package="0207/12" value="1kΩ"/>
<element name="U$2" library="coulston" package="S63P" value="10kΩ"/>
<element name="U$4" library="coulston" package="S63P" value="10kΩ"/>
<element name="U$5" library="coulston" package="S63P" value="10kΩ"/>
<element name="H1" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
</elements>
<signals>
<signal name="GND">
<contactref element="PWR" pad="P$2"/>
<contactref element="U$2" pad="LEFT"/>
<contactref element="U$4" pad="LEFT"/>
<contactref element="U$5" pad="LEFT"/>
</signal>
<signal name="VCC">
<contactref element="PWR" pad="P$1"/>
<contactref element="10MM" pad="PIN2"/>
</signal>
<signal name="GREEN_2_POT">
<contactref element="GREEN" pad="1"/>
<contactref element="U$2" pad="CENTER"/>
</signal>
<signal name="BLUE_2_POT">
<contactref element="BLUE" pad="1"/>
<contactref element="U$4" pad="CENTER"/>
</signal>
<signal name="RED_2_POT">
<contactref element="RED" pad="1"/>
<contactref element="U$5" pad="CENTER"/>
</signal>
<signal name="GREEN_2_LED">
<contactref element="GREEN" pad="2"/>
<contactref element="10MM" pad="PIN3"/>
</signal>
<signal name="BLUE_2_LED">
<contactref element="BLUE" pad="2"/>
<contactref element="10MM" pad="PIN4"/>
</signal>
<signal name="RED_2_LED">
<contactref element="RED" pad="2"/>
<contactref element="10MM" pad="PIN1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
